Telemetry CAN Communication Specification

Updated: 4 February 2016

**1 Telemetry Status**

**ID**: 0x301

**Interval:** 1000 ms

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Variable** | **Bytes** | **Type** | **Description** | |
| Unused | 7…1 | - | Unused | |
| Telemetry Status Flags | 0 | UInt8 | *Bits* | *Usage* |
| 7…2 | unused |
| 1 | 1 = COM connected |
| 0 | 1 = SQL connected |